YM16 2.022.035 Version Install Guild

1. Changes.

|  |  |
| --- | --- |
| Changes | Description |
|  |  |
|  |  |
|  |  |

1. Changes to be done.

|  |  |
| --- | --- |
| Changes | Description |
|  |  |

1. This firmware version is 2.022.035.
2. This firmware needs to be upload twice because it needs to fix reboot issue and changes firmware version.
3. Please only use Firefox or IE (no Edge) to upload this firmware.
4. This firmware does not change the current configuration file in controller.
5. Go to “System Tools” and click “Firmware Update”. Click “Browse” and choose firmware file “upload\_2\_022\_035.tar.gz”, then click “Upload”. Then click “CTRL + F5” and do the upload again. When you do the first upload, you should still see the current firmware number, and you should see the new firmware number after you upload the second time. Make sure to clear browser cache after reboot.
6. If the controller boots incorrect and web configuration still work. Please do this
   1. Change upload file name to “upload.tar.gz” and transfer the file to controller directory “/mnt/root/home/flexyard/flexyard/dfile1/” by using sftp tools (FileZilla).
   2. Use putty to connect controller through LAN1.
   3. Type command “cd /mnt/root/usr/lib/cgi-bin/configbin/” and hit enter. Then type “./uploadall.sh” and hit enter. Wait until the command finish and then reboot the board. It should fix the issue.
7. If the controller boots incorrect and web configuration does not work. Please do this
   1. Open controller’s cover and make sure the hardware jumper 2 is on
   2. Use putty and RS232 cable to connect to COMM1 on controller.
   3. Type command “cd /mnt/root/usr/lib/cgi-bin/configbin/” and hit enter. Then type “./uploadall.sh” and hit enter. Wait until the command finish and then reboot the board. It should fix the issue and the IP should come back.